No Extension Leads anywhere in or outside the House - all in Trunking
    


Day Night Sensors for Outside Lights - Front of House
Day Night Sensors for Outside Lights - Back of House 
2 sets of Battery-operated timer switches for front and back for sprinkler systems, not load shedding effected.

2 x 200-liter, 600kpa geysers on relay timer switches, never comes on simultaneously

Ceiling Trapdoors: Over and above the wood ceiling trapdoor in the passage, access to the two geysers, a further 3 white trapdoors are fitted for easy access to the reach the rest of the house. 

1 Big Red Surge Breaker fitted in Distribution Board to cover complete house

19 sets of Multiplugs
14 sets of Waterproof electrical boxes all around the house

USB plug connections in and around the house 

3 sets of LED Florescent lights in the ceiling, no lead lamps necessary.

Pool Pump fitted with Salt Water Chlorinator system – 70% functional

8 Solar Panels for the Pool

Infra-red movement sensors in every bathroom, in order to switch off the lights and ceiling extractor fans automatically. 
A similar sensor is also installed in the garage with an LED light when the sectional garage door opens.

2 x 1000-liter water tanks collecting rain water from half the roof surface and overflow runs to pool
Other half of house roof surface and also garage roof collecting water directly to pool. 

1x 1000-liter water tank with electrical pump and a pump regulator that switches on automatically when a tap is opened, to increase the water pressure into the house
Control shut off valves in down gutters from the roof of the house, can be activated to stop water flowing to pool 

In some of the rooms and living room area and also outside at braai area next to pool, the electrical wall plugs are fitted with USB connection ports

3 Air Conditioners

	Areas without an air conditioner, are fitted with ceiling fans and wall heaters





Areas without an air conditioner, are fitted with ceiling fans and wall heaters

Bathroom wall heater fitted in back room en-suite

Alarm System, throughout the house as well as in flatlet

2 Trellidoor security gates in passage way, leading to kitchen and living room

2 Trellidoor doors going out to the pool area

Coffee station with additional electrical fittings

10 Tv points, 2 DSTV points, over and above DSTV dish also additional SABC outside Aerial Grid

Foot rests, grab handles in showers

Infra-Red movement sensor on front stoop - switches on stoop light when approaching the gate at night, plus 2 lights in the passage way for one to see where to walk in the dark, switches off automatically after 3 minutes

A proper Water Purification System is installed in the kitchen.  It is a 20 liter Reverse Osmosis System

Re-chargeable bulbs and re-chargeable down lighters in the house

In the main room en-suite, installed a re-chargeable down lighter with a control switch, directly above the bathroom mirror.  This is for the lady of the house to have a bright light during load shedding, when she has to remove her make up before bed time



